**Venue Measurements**

**Listed below are the various dimensions of the Historic 512. Please give your band, DJ, caterer and service providers the measurements of the service elevator. Their equipment MUST fit through theses openings.**

|  |
| --- |
| **Facility Measurements:** |

* **Aisle:**
* 25.5 ft. long & 5ft. 5in wide
* **Outdoor Railings, 1st Floor:**
* Rails down steps 12’7
* Front 12’3
* Corners 1 1/3’
* Sides 6’10”
* Electrical Outlets at porch walls both sides
* **Staircase Railing:**
* Short railing, right side, first floor: 4’; 4’ 8” totaling 8’ 8”
* Long railing, left side, first floor: 4’; 13’ 8”; 4’1 totaling 21’ 9”
* Railing, second floor hall: 10’ 7”
* **Total railing: 41’**
* **Fireplace Mantel:**
* Wide 93” - Deep 7”- High 80”
* **KONE Elevator (service elevator):**
* 6.5’ wide; 5.5’ deep; 87” high;
* Doorway: 42” x 84”
* **OTIS Elevator (historic guest elevator):**
* 67” wide;
* 55” deep;
* 90” high;
* Doorway: 42” x 84”
* **Great Room Dimensions:**
* 46’ x’36 (east wall to archway); 36’ (fireplace to archway; 9’ (archway to stairs)
* **Grand Ballroom Dimensions: 60’ x 40’**
* Ceiling Height: 14’
* Doorways 8’ x 5’7”
* Stage Width 21’3”
* Stage Height (to frame) 9’2”
* Stage Length 16’4”
* **Parlor B (Bride’s Room):** 25’ x 14’
* **Bishop Parlor (Groom’s Room):** 25’ x 14’

**Reminders:**

 **Renters may not move furniture between floors.**

 **No outside rental tables or chairs are allowed in building unless from an approved source.**